2D frozen spin method for search for the deuteron electric dipole moment using storage ring

Alexander Aksentyev1,2,3\*, Yury Senichev1,Eremey Valetov4,  
1 Institute for Nuclear Research of the Russian Academy of Sciences, Moscow, Russia  
2 Institut für Kernphysik, Forschungszentrum Jülich, Jülich, Germany  
3 National Research Nuclear University “MEPhI,” Moscow, Russia  
4 Department of Physics and Astronomy, Michigan State University, East Lansing, Michigan, USA

**Email address:**

[y.senichev@inr.ru](mailto:y.senichev@inr.ru) (Yury Senichev)

[alexaksentyev@gmail.com](mailto:alexaksentyev@gmail.com) (Alexander Aksentyev)

[eremey@valetov.com](mailto:eremey@valetov.com) (Eremey Valetov)

* Corresponding author

**Abstract:**

The proposed method aims at suppressing the geometric phase  and machine imperfection  systematic errors, which are encountered in any frozen spin storage ring EDM measurement method based on observation of a slow, gradual change in the beam polarisation vector. The geometric phase error s caused by non-commutating wobbling precessions of the polarisation vector, which are significant only if the polarisation vector precession rate is small. Geometric phase can be suppressed by dispensing with operating in the spin resonance (i.e., 3D Frozen Spin) state, in favour of the 2D FS state, represented by a rolling spin wheel.  To eliminate the machine imperfection systematic error, the imperfection fields themselves are utilised as the drivers of the spin wheel. The method is intended for a combined storage ring; the bend fields are magnetic and the frozen spin condition is met using multiple, uniformly-distributed, Wien filters. Reversing the bending field (along with the beam direction) reverses the imperfection fields. The EDM measurement consists of measuring the difference of spin wheel roll rates, which is proportional to the EDM. Though motivated by the need to measure the deuteron EDM, the method can also be applied to the proton.

**Keywords:** electric dipole moment, frequency domain, space domain, geometric phase error, imperfect lattice, storage ring

# 1. Motivation

Storage ring-based methods of search for the electric dipole moments (EDMs) of fundamental particles can be classified into two major categories, which we will call *a*) Space Domain, and *b*) Frequency Domain methods.

In the Space Domain paradigm, one measures a *change in the spatial orientation* of the beam polarisation vector *caused by the EDM*.

The original storage ring, frozen spin-type method, proposed in [1], is a canonical example of a methodology in the space domain: an initially longitudinally-polarised beam is injected into the storage ring; the vertical component of its polarisation vector is observed. Under ideal conditions, any tilting of the beam polarisation vector from the horizontal plane is attributed to the action of the EDM.

Two technical difficulties are readily apparent with this approach:

1. it poses a challenging task for polarimetry [2];
2. it puts very stringent constraints on the precision of the accelerator optical element alignment.

The former is due to the requirement of detecting a change of about to the cross section asymmetry in order to get to the EDM sensitivity level of . [1, p. 18]

The latter is to minimise the magnitude of the vertical plane magnetic dipole moment (MDM) precession frequency: [1, p. 11]

|  |  |
| --- | --- |
|  | (1) |

induced by machine imperfection fields. According to estimates done by Y. Senichev, if it is to be fulfilled, the geodetic installation precision of accelerator elements must reach m. Today’s technology allows only for about m.

At the practically-achievable level of element alignment uncertainty, , and changes in the orientation of the polarisation vector are no longer EDM-driven.

Another crucial problem one faces in the space domain is geometric phase error. [3, p. 6] The problem here lies in the fact that, even if one can somehow make field imperfections (either due to optical element misalignment or spurious electro-magnetic fields) zero *on average*, since spin rotations are non-commutative, the polarisation rotation angle due to them will not be zero.

By contrast, the Frequency Domain methodology is founded on measuring the EDM *contribution* to the total (MDM and EDM together) spin precession *angular velocity*.

The polarisation vector is made to roll about a nearly-constant, definite direction vector , with an angular velocity that is high enough for its magnitude to be easily measurable at all times. Apart from easier polarimetry, the definiteness of the angular velocity vector is a safeguard against geometric phase error.

This “Spin Wheel” may be externally applied [4], or otherwise the machine imperfection fields may be utilised for the same purpose (wheel roll rate determined by equation (1)). The latter is made possible by the fact that changes sign when the beam revolution direction is reversed. [1, p. 11]

# 2. Universal SR EDM measurement problems

By way of introduction to the proposed measurement methodology, let us briefly summarise some measurement problems encountered by any EDM experiment performed in a storage ring; they can be grouped into two big categories:

* Problems solved by a Spin Wheel:
  + spurious electro-magnetic fields;
  + betatron motion.
* Problems having specific solutions:
  + spin decoherence;
  + machine imperfections.

## 2.1 Spin motion perturbation

Problems from the first category are ones introducing geometric phase error. Indeed, both the spurious and the focusing fields, when acting on a betatron-oscillating particle, perturb the direction and magnitude of its spin precession angular velocity vector. The effect is a spin kick in the direction defined by the perturbation.

Assume that the EDM provides a spin kick about the radial (-) axis. The magnitude of the angular velocity vector has a general form

where is minimised by fulfilling the frozen spin condition; (the constant part of which is due to machine imperfections) can be minimised via the installation of a longitudinal solenoid on the optic axis. (1 m long, magnetic field approximately T.) In the space domain, one also tries to minimise the contribution to . Consequently, spin kicks must be minimised to (significantly) less than , so as to reduce geometric phase to less than the accumulated EDM phase.

The benefit of having a Spin Wheel aligned with the EDM angular velocity is that orthogonal MDM contributions to the total angular velocity vector add up in squares, and hence their effect is greatly diminished:

Since our goal is to observe the EDM-related value shift in , we need to minimise random variable :

Let’s make some preliminary estimates. Suppose rad/sec (the reason for choosing this value will be explained shortly), rad/sec (corresponding to the EDM value cm). Then, must be reduced to less than rad/sec, or equivalently, either angular velocity to less than rad/sec. This is several orders of magnitude greater than the expected standard error on the angular velocity estimate, [5] and hence should not be a problem to achieve.

One case left to be considered is MDM spin kicks about the -axis. These are not attenuated, and cause the most trouble. They come in three varieties: *a*) permanent, not caused by optical element misalignments; *b*) semi-permanent, caused by element tilts about the optic axis; *c*) spurious.

Semi-permanent radial spin kicks (be they caused by magnetic or electric fields) change sign when the beam revolution direction is reversed from clockwise (CW) to counter-clockwise (CCW). Spurious kicks can be dealt with by statistical averaging. Permanent, insensitive to either the guide field or the beam circulation direction, cannot be controlled. On the bright side, their sources should not be present under normal circumstances.

For more details on spin motion perturbation effects on the measurement of the EDM in frequency domain, please refer to [6].

## 2.2 Expected machine imperfection SW roll rate

In the estimates above, we used a roll rate rad/sec for the spin wheel. This is our expected caused by machine imperfections.

Denote the standard deviation of the imperfection radial magnetic field distribution . For the whole ring, MDM precession will be distributed with a standard deviation [7]

where is the number of misaligned elements, is the anomalous magnetic dipole moment.

For deuterons in lattices [8] of on the order of 100 elements, rotated about the optic axis by angles rad, Y. Senichev estimates [7] between 50 and 100 rad/sec.

Our simulations done in COSY INFINITY seem to confirm this result. In Figure 1 you see the results of the simulation in which we rotated the 32 E+B spin rotator elements used in the frozen spin (codename BNL) lattice [8] by angles randomly picked from the distribution , where rad, .




Figure 1. Spin precession frequency (radial and vertical components) versus the mean E+B element tilt angle

At we observe a roll rate of 500 rad/sec. We should keep in mind, however, that Senichev assumes rad, which means, for a lattice with tilted elements, a standard deviation of the mean . The dependence of on is linear, which means in an actual lattice we would observe an rad/sec with 68% probability, and rad/sec with 95% probability, and with 27% probability .

## 2.3 Spin decoherence

Spin coherence is a measure or quality of preservation of polarisation in an initially fully-polarised beam. [9] Spin decoherence refers to the depolarisation caused by the difference in the beam particles’ spin precession frequencies.

The difference in spin tunes is due to the difference of the particles’ orbit lengths, and hence their equilibrium energy levels, on which spin tune depends. One way spin decoherence can be suppressed is by utilisation of sextupole fields. We consider how this can be accomplished in [10].

## 2.4 Machine imperfections

As we have seen, the problem with machine imperfections is twofold: *a*) they are practically impossible to remove at the present level of technology; but what’s even worse, *b*) their removal leaves one in the space domain, and opens the measurement up to geometric phase error.

Fortunately for us, the imperfection spin kicks they induce change sign when the beam circulation direction is reversed. Their magnitude is also sufficient for use as a Koop Wheel. The one remaining difficulty is the accuracy of the Koop wheel roll direction flipping. Hopefully, we can make a persuasive enough argument as to how this can accomplished.

# 3. Main methodology features

The method we propose is characterised by two main features:

1. It is a frequency domain method;
2. The fields induced by machine imperfections, instead of being suppressed, are used as a Koop Wheel.
   * The Koop Wheel roll direction is reversed by flipping the direction of the guide field;
   * its roll rate is controlled through observation of spin precession in the horizontal plane.

The advantages of the frequency domain, such as *a*) ease of polarimetry, and *b*) immunity to geometric phase error, have been discussed in previous sections. Now we will turn to the description of how machine imperfection fields can be used as a Koop Wheel.

# 4. EDM estimator statistic

Since the angular velocity measured in the frequency domain methodology includes contributions due to both the magnetic and electric dipole moments, the EDM estimator statistic requires two cycles to compose: one in which the Koop Wheel rolls forward, the other backward.

The change in the Koop Wheel roll direction is affected by flipping the direction of the guide field. When this is done: , the beam circulation direction changes from clockwise (CW) to counter-clockwise (CCW): , while the electrostatic field remains constant: . According to the T-BMT equation, spin precession frequency components change like:

|  |  |
| --- | --- |
|  |  |
|  |  |
|  | (2a) |

And the EDM estimator

|  |  |
| --- | --- |
|  | (2b) |
|  | (2c) |

To keep the systematic error term below required precision, i.e. ensure that equation (2a) holds with sufficient accuracy, Y. Senichev devised [7] a guide field flipping procedure based on observation of the beam polarisation precession frequency in the horizontal plane.

To explain how it works, we need to introduce the concept of the effective Lorentz factor.

# 5. Effective Lorentz factor

Spin dynamics is described by the concepts of *spin tune* and *invariant spin axis* . Spin tune depends on the particle’s equilibrium-level energy, expressed by the Lorentz factor:

|  |  |
| --- | --- |
|  | (3) |

Unfortunately, not all beam particles share the same Lorentz factor. A particle involved in betatron motion will have a longer orbit, and as a direct consequence of the phase stability principle, in an accelerating structure utilising an RF cavity, its equilibrium energy level must increase. Otherwise it cannot remain the bunch. In this section we analyse how the particle Lorentz factor should be modified when betatron motion, as well as non-linearities in the momentum compaction factor are accounted for.

The longitudinal dynamics of a particle on the reference orbit of a storage ring is described by the system of equations:

|  |  |
| --- | --- |
|  | (4) |

In the equations above, and are the deviations of the particle’s phase and normalised momentum from those of the reference particle, and are the RF cavity frequency and voltage, is the harmonic number, is the slip-factor, is the particle’s relative velocity factor, and is its total energy.

The solutions of this system form a family of ellipses in the -plane, all centered at the point . However, if one considers a particle involved in betatron oscillations, and uses a higher-order Taylor expansion of the momentum compaction factor , the first equation of the system transforms into: [11, p. 2579]

where, is the betatron motion-related orbit lengthening; and are the horizontal and vertical beam emittances, and , are the horizontal and vertical tunes.

The solutions of the transformed system are no longer centered at the same single point. Orbit lengthening and momentum deviation cause an equilibrium-level momentum shift [11, p.2581]

|  |  |
| --- | --- |
|  | (5) |

where is the amplitude of synchrotron oscillations.

|  |  |
| --- | --- |
|  | (6) |

We call the equilibrium energy level associated with the momentum shift , the *effective Lorentz factor:*

where , are the Lorentz factor and relative velocity factor of the reference particle.

Observe, that the effective Lorentz factor enables us to account for variation in the value of spin tune due to variation in the particle orbit length. It is crucial in the analysis of spin decoherence [10]  and its suppression by means of sextupole fields.

It plays a big role, as well, in the successful reproduction of the MDM component to the total spin precession angular velocity.

# 6. Guide field flipping

Two aspects of the problem require attention:

1. What needs to be kept constant from one measurement cycle to the next;
2. How it can be observed.

The goal of flipping the direction of the guide field is to accurately reproduce the radial component of the MDM spin precession frequency induced by machine imperfection fields. This point should not be overlooked: a mere reproduction of the *magnetic field strength* would not suffice, since the injection point of the beam’s centroid, and hence its orbit length — and, via equations (6) and (3), spin tune, — is subject to variation. (Apart from that, the accelerating structure might not be symmetrical, in terms of spin dynamics, with regard to reversal of the beam circulation direction.)

What needs to be reproduced, therefore, is not the field strength, but the effective Lorentz factor of the centroid.

Regarding the second question, we mentioned earlier that the Koop Wheel roll rate is controlled through measurement of the horizontal plane spin precession frequency. This plane was chosen because the EDM angular velocity vector points (mainly) in the radial direction; its vertical component is due to machine imperfection fields, and is small compared to the measured EDM effect. Therefore, in first approximation, when we manipulate the vertical component of the combined spin precession angular velocity, we manipulate the vertical component of the MDM angular velocity vector.

Moving on to the effective Lorentz factor calibration procedure. Let denote the set of all trajectories that a particle might follow in the accelerator. , where is the set of all stable trajectories, are all trajectories such that if a particle gets on one, it will be lost from the bunch.

Calibration is done in two phases:

1. In the first phase, the guide field value is set so that the beam particles are injected onto trajectories .
2. In the second phase, it is fine-tuned further, so as to fulfil the FS condition in the horizontal plane. By doing this, we physically move the beam trajectories into the subset of trajectories for which .

Spin tune (and hence precession frequency) is an injective function of the effective Lorentz-factor , which means. The trajectory space is partitioned into equivalence classes according to the value of: trajectories characterised by the same are equivalent in terms of their spin dynamics (possess the same spin tune and invariant spin axis direction), and hence belong to the same equivalence class. Since is injective, there exists a unique at which :

.

If the lattice didn’t use sextupole fields for the suppression of decoherence, would be a singleton set. We have shown in [10] that if sextupoles are utilised, then such that: , . By adjusting the guide field strength we equate , and hence contains multiple trajectories. (Strictly speaking, even if sextupoles are used there remains some negligible dependence of spin tune on the particle orbit length (linear decoherence effects, cf. [10]). Because of that, the equalities for and are approximate, and the set should be viewed as fuzzy: we will consider trajectories for which for some small as belonging to .)

Therefore, once we ensured that the beam polarisation does not precess in the horizontal plane, all of the beam particles have , equal for the CW and CCW beams.

Guide field flipping procedure simulation results can be found in [12].

# 7. Statistical precision

Members of the JEDI Collaboration have studied the statistical precision of spin precession angular velocity estimation from sparse (one detector event per 100 spin revolutions) [13] and dense [5] polarisation data.

According to [13], the maximum likelihood estimator for the spin precession frequency estimate has a standard error

where is the total number of recorded detector events, is the beam polarisation, is the measurement time.

Assuming events, polarisation , and cycle duration seconds (same parameters as in the simulation done in [5]), we have rad/sec at the cycle level. Estimates made in [5] agree with this result.

This precision is sufficient to obtain a mean estimate with statistical uncertainty rad/sec in one year of measurement, with the accelerator operational 70% of the time. An EDM of cm should induce an on the level of rad/sec in storage rings proposed in [8]. Thus, we expect to be able to measure the deuteron EDM at the cm level in one year of measurement time.

# References

[1] D. Anastassopoulos et al., “AGS Proposal: Search for a permanent electric dipole moment of the deuteron nucleus at the ecm level,” BNL, 2008.

[2] S. Mane, “A distillation of Koop’s idea of the Spin Wheel,” arXiv:1509.01167 [physics] <http://arxiv.org/abs/1509.01167>.

[3] V. Anastassopoulos et al., “A Storage Ring Experiment to Detect a Proton Electric Dipole Moment.” Rev. Sci. Instrum., 87(11), 2016. <http://arxiv.org/abs/1502.04317>.

[4] I. Koop. “Asymmetric energy colliding ion beams in the EDM storage ring,” Proc. of IPAC13 (2013). <http://accelconf.web.cern.ch/accelconf/ipac2013/papers/tupwo040.pdf>.

[5] A. Aksentev, Y. Senichev. “Statistical precision in charged particle EDM search in storage rings.” 2017 J. Phys.: Conf. Ser. 941 012083.

[6] A. Aksentev, Y. Senichev, “Spin Motion Perturbation Effect on the EDM Statistic in the Frequency Domain Method,” presented at the 10th International Particle Accelerator Conf. (IPAC’19), Melbourne, Australia, May. 2019, paper MOPTS011.

[7] Y. Senichev, A. Aksentev, A. Ivanov, E. Valetov, “Frequency domain method of the search for the deuteron electric dipole moment in a storage ring with imperfections,” arxiv:1711.06512 [physics.acc-ph] <https://arxiv.org/abs/1711.06512>.

[8] Y. Senichev, S. Andrianov, S. Chekmenev, M. Berz, E.Valetov. “Investigation of Lattice for Deuteron EDM Ring,” Proc. of ICAP15 (2015). <http://accelconf.web.cern.ch/AccelConf/ICAP2015/papers/modbc4.pdf>.

[9] E. Valetov, “Field modeling, symplectic tracking, and spin decoherence for the EDM and muon g-2 lattices.” PhD tehsis, Michigan State University, Michigan, USA. <http://collaborations.fz-juelich.de/ikp/jedi/public_files/theses/valetovphd.pdf>.

[10] A. Aksentev, Y. Senichev, “Spin decoherence in the Frequency Domain Method for the search of a particle EDM,” presented at the 10th International Particle Accelerator Conf. (IPAC’19), Melbourne, Australia, May. 2019, paper MOPTS012.

[11] Y. Senichev et al., “Spin tune decoherence effects in Electro- and Magnetostatic Structures.” Proceedings of IPAC 2013, Shanghai, China, pp. 2579-2581.

[12] A. Aksentev, Y. Senichev, “Simulation of the Guide Field Flipping Procedure for the Frequency Domain Method,” presented at the 10th International Particle Accelerator Conf. (IPAC’19), Melbourne, Australia, May 2019, paper MOPTS010.

[13] J. Pretz, “Determination of polarization and frequency parameters on sparse data,” JEDI internal note #2013/04, Sept. 23, 2013.